(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "1437566-3"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at -3.8125 2.5417 0)
		)
		(property "Value" "1437566-3"
			(at -3.8141 -3.8141 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:1437566-3"
			(at 0.254 5.334 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "FSMSM=3.5X6 SMT TACT | TE Connectivity 1437566-3"
			(at 0.254 5.334 0)
		)
		(property "Comment" "1437566-3"
			(at 0 0 0)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/1437566-3/TE+Connectivity+ALCOSWITCH+Switches/view-part/?ref=snap"
			(at 0.254 5.334 0)
		)
		(property "Manufacturer PN" "1437566-3"
			(at 0 0 0)
		)
		(property "Manufacturer" "TE CONNECTIVITY"
			(at 0 0 0)
		)
		(symbol "1437566-3_0_0"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "2SC3356"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 7.874 0)
		)
		(property "Value" "2SC3356"
			(at -4.064 5.842 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-3"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Transistor NPN, RF 12 GHz"
			(at 0 0 0)
		)
		(property "Manufacturer" "EVVO"
			(at 0 0 0)
		)
		(property "Manufacturer PN" "2SC3356"
			(at 0 0 0)
		)
		(symbol "2SC3356_0_1")
		(symbol "2SC3356_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin open_collector line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin open_emitter line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "691411510002"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -4.99 -1.205 0)
		)
		(property "Value" "691411510002"
			(at -4.95 -3.01 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:691411510002"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "2 Position wire to board Terminal Block"
			(at 0 0 0)
		)
		(property "Manufacturer PN" "691411510002"
			(at 0 0 0)
		)
		(property "Manufacturer" "Wurth Elektronik"
			(at 0 0 0)
		)
		(symbol "691411510002_0_0"
			(pin passive line
				(at -2.54 -5.08 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "A1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "A2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ABS07-32.768KHZ-T"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at 8.89 6.35 0)
		)
		(property "Value" "ABS07-32.768KHZ-T"
			(at 8.89 3.81 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:ABS07"
			(at 8.89 -96.19 0)
		)
		(property "Datasheet" "https://abracon.com/Resonators/ABS07.pdf"
			(at 8.89 -196.19 0)
		)
		(property "Description" "32.768 kHz +/-20ppm Crystal 7pF 70 kOhms 2-SMD, No Lead"
			(at 0 0 0)
		)
		(property "Height" "0.9"
			(at 8.89 -396.19 0)
		)
		(property "Mouser Part Number" "815-ABS07-32.768KHZT"
			(at 8.89 -496.19 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/ABRACON/ABS07-32.768KHZ-T?qs=3SpAxaLJ01g8GJWeO3sA3Q%3D%3D"
			(at 8.89 -596.19 0)
		)
		(property "Manufacturer" "ABRACON"
			(at 8.89 -696.19 0)
		)
		(property "Manufacturer PN" "ABS07-32.768KHZ-T"
			(at 8.89 -796.19 0)
		)
		(symbol "ABS07-32.768KHZ-T_1_1"
			(pin passive line
				(at 0 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8592"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 16.764 0)
		)
		(property "Value" "AD8592"
			(at 0 0 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:AD8592"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Standard (General Purpose) Amplifier 2 Circuit Rail-to-Rail 10-MSOP"
			(at 0 0 0)
		)
		(property "Manufacturer" "Analog Devices Inc."
			(at 0 0 0)
		)
		(property "Manufacturer PN" "AD8592ARMZ-REEL"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "AD8592_0_1")
		(symbol "AD8592_1_1"
			(pin input line
				(at 5.08 11.43 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at 5.08 6.35 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at 10.16 16.51 270)
				(length 3.81)
				(name "V+")
				(number "10")
			)
			(pin power_in line
				(at 10.16 1.27 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 12.7 2.54 90)
				(length 3.81)
				(name "~{SD}")
				(number "5")
			)
			(pin output line
				(at 20.32 8.89 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "AD8592_2_1"
			(pin input line
				(at 5.08 11.43 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin input line
				(at 5.08 6.35 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin power_in line
				(at 10.16 16.51 270)
				(length 3.81)
				(name "V+")
				(number "10")
			)
			(pin power_in line
				(at 10.16 1.27 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 12.7 2.54 90)
				(length 3.81)
				(name "~{SD}")
				(number "6")
			)
			(pin output line
				(at 20.32 8.89 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP2112K-3.3TRG1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 26.67 7.62 0)
		)
		(property "Value" "AP2112K-3.3TRG1"
			(at 26.67 5.08 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:AP2112K-3.3TRG1"
			(at 26.67 -94.92 0)
		)
		(property "Datasheet" "https://www.diodes.com//assets/Datasheets/AP2112.pdf"
			(at 26.67 -194.92 0)
		)
		(property "Description" "600mA 3.3V LDO Regulator Enable SOT23-5 DiodesZetex AP2112K-3.3TRG1, LDO Voltage Regulator, 3.3 V +/-1.5%, 2.5  6 Vin, 5-Pin SOT-23"
			(at 0 0 0)
		)
		(property "Height" "1.4"
			(at 26.67 -394.92 0)
		)
		(property "Mouser Part Number" "621-AP2112K-3.3TRG1"
			(at 26.67 -494.92 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/AP2112K-3.3TRG1?qs=x6A8l6qLYDDPYHosCdzh%2FA%3D%3D"
			(at 26.67 -594.92 0)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 26.67 -694.92 0)
		)
		(property "Manufacturer PN" "AP2112K-3.3TRG1"
			(at 26.67 -794.92 0)
		)
		(symbol "AP2112K-3.3TRG1_1_1"
			(pin power_in line
				(at 0 0 0)
				(length 5.08)
				(name "VIN")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 0)
				(length 5.08)
				(name "EN")
				(number "3")
			)
			(pin power_out line
				(at 30.48 0 180)
				(length 5.08)
				(name "VOUT")
				(number "5")
			)
			(pin no_connect line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at 30.48 -6.35 180)
				(length 5.08)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APG1608CGKC_T"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 12.7 8.89 0)
		)
		(property "Value" "APG1608CGKC_T"
			(at 12.7 6.35 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:APG1608CGKC_T"
			(at 12.7 -93.65 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/APG1608CGKC-T.pdf"
			(at 12.7 -193.65 0)
		)
		(property "Description" "2.6 V Green LED 1608 (0603) SMD, Kingbright APG1608CGKC/T"
			(at 0 0 0)
		)
		(property "Height" "0.28"
			(at 12.7 -393.65 0)
		)
		(property "Mouser Part Number" "604-APG1608CGKC/T"
			(at 12.7 -493.65 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Kingbright/APG1608CGKC-T?qs=uxmOeTEqoPwOMdoDiWi4nA%3D%3D"
			(at 12.7 -593.65 0)
		)
		(property "Manufacturer" "Kingbright"
			(at 12.7 -693.65 0)
		)
		(property "Manufacturer PN" "APG1608CGKC/T"
			(at 12.7 -793.65 0)
		)
		(symbol "APG1608CGKC_T_0_1")
		(symbol "APG1608CGKC_T_1_1"
			(pin passive line
				(at 3.81 2.54 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 11.43 2.54 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BAV99,215"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 12.7 10.16 0)
		)
		(property "Value" "BAV99,215"
			(at 12.7 7.62 0)
		)
		(property "Footprint" "BAV99215"
			(at 12.7 -92.38 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV99_SER.pdf"
			(at 12.7 -192.38 0)
		)
		(property "Description" "Diodes - General Purpose, Power, Switching SW DBL 75V 215MA HS"
			(at 0 0 0)
		)
		(property "Height" "1.1"
			(at 12.7 -392.38 0)
		)
		(property "Mouser Part Number" "771-BAV99-T/R"
			(at 12.7 -492.38 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Nexperia/BAV99215?qs=me8TqzrmIYWbN0bCKV3n5w%3D%3D"
			(at 12.7 -592.38 0)
		)
		(property "Manufacturer" "Nexperia"
			(at 12.7 -692.38 0)
		)
		(property "Manufacturer PN" "BAV99,215"
			(at 12.7 -792.38 0)
		)
		(symbol "BAV99,215_1_1"
			(pin passive line
				(at 0 0 0)
				(length 5.08)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 0)
				(length 5.08)
				(name "E")
				(number "2")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-C3-WROOM-02U-N4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 5.588 7.112 0)
		)
		(property "Value" "ESP32-C3-WROOM-02U-N4"
			(at 5.334 4.572 0)
		)
		(property "Footprint" "ESP32C3WROOM02UN4"
			(at 29.21 -94.92 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-c3-wroom-02_datasheet_en.pdf"
			(at 29.21 -194.92 0)
		)
		(property "Description" "Multiprotocol Modules SMD module, ESP32-C3, 4MB SPI flash, IPEX antenna, -40 C +85 C"
			(at 0 0 0)
		)
		(property "Height" "3.35"
			(at 29.21 -394.92 0)
		)
		(property "Mouser Part Number" "356-ESP32C3WROM02UN4"
			(at 29.21 -494.92 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Espressif-Systems/ESP32-C3-WROOM-02U-N4?qs=pBJMDPsKWf2Ces2aXBSNjQ%3D%3D"
			(at 29.21 -594.92 0)
		)
		(property "Manufacturer" "Espressif Systems"
			(at 29.21 -694.92 0)
		)
		(property "Manufacturer PN" "ESP32-C3-WROOM-02U-N4"
			(at 29.21 -794.92 0)
		)
		(symbol "ESP32-C3-WROOM-02U-N4_1_1"
			(pin passive line
				(at 0 0 0)
				(length 5.08)
				(name "3V3")
				(number "1")
			)
			(pin passive line
				(at 0 -2.54 0)
				(length 5.08)
				(name "EN")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 0)
				(length 5.08)
				(name "IO4")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 0)
				(length 5.08)
				(name "IO5")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 0)
				(length 5.08)
				(name "IO6")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 0)
				(length 5.08)
				(name "IO7")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 0)
				(length 5.08)
				(name "IO8")
				(number "7")
			)
			(pin passive line
				(at 0 -17.78 0)
				(length 5.08)
				(name "IO9")
				(number "8")
			)
			(pin passive line
				(at 0 -20.32 0)
				(length 5.08)
				(name "IO10")
				(number "10")
			)
			(pin passive line
				(at 0 -22.86 0)
				(length 5.08)
				(name "RXD")
				(number "11")
			)
			(pin passive line
				(at 0 -25.4 0)
				(length 5.08)
				(name "TXD")
				(number "12")
			)
			(pin passive line
				(at 33.02 0 180)
				(length 5.08)
				(name "IO18")
				(number "13")
			)
			(pin passive line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "IO19")
				(number "14")
			)
			(pin passive line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "IO3")
				(number "15")
			)
			(pin passive line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "IO2")
				(number "16")
			)
			(pin passive line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "IO1")
				(number "17")
			)
			(pin passive line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "IO0")
				(number "18")
			)
			(pin passive line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "EPAD")
				(number "19")
			)
			(pin passive line
				(at 33.02 -22.86 180)
				(length 5.08)
				(hide yes)
				(name "GND_3")
				(number "20")
			)
			(pin passive line
				(at 33.02 -22.86 180)
				(length 5.08)
				(hide yes)
				(name "GND_4")
				(number "21")
			)
			(pin passive line
				(at 33.02 -22.86 180)
				(length 5.08)
				(hide yes)
				(name "GND_5")
				(number "22")
			)
			(pin passive line
				(at 33.02 -22.86 180)
				(length 5.08)
				(hide yes)
				(name "GND_6")
				(number "23")
			)
			(pin passive line
				(at 33.02 -22.86 180)
				(length 5.08)
				(hide yes)
				(name "GND_7")
				(number "24")
			)
			(pin passive line
				(at 33.02 -22.86 180)
				(length 5.08)
				(hide yes)
				(name "GND_8")
				(number "25")
			)
			(pin passive line
				(at 33.02 -22.86 180)
				(length 5.08)
				(hide yes)
				(name "GND_9")
				(number "26")
			)
			(pin passive line
				(at 33.02 -22.86 180)
				(length 5.08)
				(hide yes)
				(name "GND_10")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EXB28V331JX"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at 15.24 8.89 0)
		)
		(property "Value" "EXB28V331JX"
			(at 15.24 6.35 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:EXB28V331JX"
			(at 0 0 0)
		)
		(property "Datasheet" "EXB28V331JX"
			(at 0 0 0)
		)
		(property "Description" "Resistor Array, 0804"
			(at 0 0 0)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 0)
		)
		(property "Manufacturer PN" "EXB28V331JX"
			(at 0 0 0)
		)
		(property "ki_keywords" "EXB28V331JX"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "C_ARRAY_EXB28V_PAN C_ARRAY_EXB28V_PAN-M C_ARRAY_EXB28V_PAN-L"
			(at 0 0 0)
		)
		(symbol "EXB28V331JX_0_1"
			(pin passive line
				(at 0 0 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 0)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 30.48 0 180)
				(length 7.62)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at 30.48 -5.08 180)
				(length 7.62)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at 30.48 -10.16 180)
				(length 7.62)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at 30.48 -15.24 180)
				(length 7.62)
				(name "5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IHLP1616ABER1R0M01"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "L"
			(at 16.51 6.35 0)
		)
		(property "Value" "IHLP1616ABER1R0M01"
			(at 16.51 3.81 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:INDPM4441X200N"
			(at 16.51 -96.19 0)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/2/IHLP1616ABER1R0M01.pdf"
			(at 16.51 -196.19 0)
		)
		(property "Description" "Fixed Inductors 1uH 20%"
			(at 0 0 0)
		)
		(property "Height" "2"
			(at 16.51 -396.19 0)
		)
		(property "Manufacturer" "Vishay"
			(at 16.51 -696.19 0)
		)
		(property "Manufacturer PN" "IHLP1616ABER1R0M01"
			(at 16.51 -796.19 0)
		)
		(symbol "IHLP1616ABER1R0M01_1_1"
			(pin passive line
				(at 0 0 0)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 5.08)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INND-TS30RAB"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 20.32 10.16 0)
		)
		(property "Value" "INND-TS30RAB"
			(at 20.32 7.62 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:INND-TS30RAB"
			(at 0 7.62 0)
		)
		(property "Datasheet" "INND-TS30RAB"
			(at 0 7.62 0)
		)
		(property "Description" "7-segment display"
			(at 0 0 0)
		)
		(property "Manufacturer" "Inolux"
			(at 0 0 0)
		)
		(property "Manufacturer PN" "INND-TS30RAB"
			(at 0 0 0)
		)
		(property "ki_keywords" "INND-TS30RAB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT10_INND-TS30RAB_INL"
			(at 0 0 0)
		)
		(symbol "INND-TS30RAB_0_1")
		(symbol "INND-TS30RAB_1_1"
			(pin passive line
				(at 0 3.81 0)
				(length 7.62)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 0 1.27 0)
				(length 7.62)
				(name "B")
				(number "9")
			)
			(pin passive line
				(at 0 -1.27 0)
				(length 7.62)
				(name "C")
				(number "8")
			)
			(pin passive line
				(at 0 -3.81 0)
				(length 7.62)
				(name "D")
				(number "5")
			)
			(pin passive line
				(at 0 -6.35 0)
				(length 7.62)
				(name "E")
				(number "4")
			)
			(pin passive line
				(at 0 -8.89 0)
				(length 7.62)
				(name "F")
				(number "3")
			)
			(pin passive line
				(at 0 -11.43 0)
				(length 7.62)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 0 -13.97 0)
				(length 7.62)
				(name "DP")
				(number "7")
			)
			(pin passive line
				(at 40.64 2.54 180)
				(length 7.62)
				(name "AN")
				(number "1")
			)
			(pin passive line
				(at 40.64 0 180)
				(length 7.62)
				(name "AN")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LQW18CNR27J00D"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "L"
			(at 16.51 6.35 0)
		)
		(property "Value" "LQW18CNR27J00D"
			(at 16.51 3.81 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:LQM18PH1R0MFRL"
			(at 16.51 -96.19 0)
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/P02/JELF243A-0082.pdf"
			(at 16.51 -196.19 0)
		)
		(property "Description" "Murata LQW18CN_00 Series Wire-wound SMD Inductor with a Ferrite Core, 270 nH Wire-Wound 750mA Idc"
			(at 0 0 0)
		)
		(property "Height" "0.95"
			(at 16.51 -396.19 0)
		)
		(property "Manufacturer" "Murata Electronics"
			(at 16.51 -696.19 0)
		)
		(property "Manufacturer PN" "LQW18CNR27J00D"
			(at 16.51 -796.19 0)
		)
		(symbol "LQW18CNR27J00D_1_1"
			(pin passive line
				(at 0 0 0)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 5.08)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PTV09A-4020U-B104"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -5.08 5.334 0)
		)
		(property "Value" "PTV09A-4020U-B104"
			(at -8.382 0.762 90)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:PTV09A4020FBxxx"
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Potentiometer, US symbol"
			(at -0.762 14.732 0)
		)
		(property "Manufacturer PN" "PTV09A-4020U-B104"
			(at -3.302 13.208 0)
		)
		(property "Manufacturer" "Bourns"
			(at 5.588 11.176 0)
		)
		(property "ki_keywords" "resistor variable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Potentiometer*"
			(at 0 0 0)
		)
		(symbol "PTV09A-4020U-B104_0_1")
		(symbol "PTV09A-4020U-B104_1_1"
			(text "MNT"
				(at -3.81 -0.254 900)
			)
			(pin power_in line
				(at -3.81 -6.35 90)
				(length 3.81)
				(name "MNT")
				(number "4")
			)
			(pin power_in line
				(at -3.81 -6.35 90)
				(length 3.81)
				(hide yes)
				(name "MNT")
				(number "5")
			)
			(pin passive line
				(at 0 6.35 270)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -6.35 90)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 6.35 0 180)
				(length 3.81)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "S2B-XH-A_LF_SN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -2.544 2.544 0)
		)
		(property "Value" "S2B-XH-A_LF_SN"
			(at -2.5433 -3.8149 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:JST_S2B-XH-A_LF__SN_"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Connector Header Through Hole, Right Angle 2 position 0.098 (2.50mm)"
			(at 0 0 0)
		)
		(property "MF" "JST Sales"
			(at 0 0 0)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/S2B-XH-A%20(LF)(SN)/JST/view-part/?ref=snap"
			(at 0 0 0)
		)
		(property "Manufacturer PN" "S2B-XH-A (LF)(SN)"
			(at 0 0 0)
		)
		(property "Manufacturer" "JST"
			(at 0 0 0)
		)
		(symbol "S2B-XH-A_LF_SN_0_0"
			(pin passive line
				(at -7.62 1.27 0)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 -1.27 0)
				(length 5.08)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SI4844-B20-GU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 29.21 7.62 0)
		)
		(property "Value" "SI4844-B20-GU"
			(at 29.21 5.08 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:SI4844-B20-GU"
			(at 29.21 -94.92 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/SkyWorks/SL/documents/public/data-sheets/Si4844-B20.pdf"
			(at 29.21 -194.92 0)
		)
		(property "Description" "RF Receiver FM/AM/SW-wide band with mechanical tuning/digital display"
			(at 0 0 0)
		)
		(property "Height" "1.75"
			(at 29.21 -394.92 0)
		)
		(property "Manufacturer" "Skyworks"
			(at 29.21 -494.92 0)
		)
		(property "Manufacturer PN" "SI4844-B20-GU"
			(at 29.21 -594.92 0)
		)
		(symbol "SI4844-B20-GU_1_1"
			(pin passive line
				(at 0 0 0)
				(length 5.08)
				(name "LNA_EN")
				(number "1")
			)
			(pin output line
				(at 0 -2.54 0)
				(length 5.08)
				(name "IRQ")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 0)
				(length 5.08)
				(name "TUNE1")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 0)
				(length 5.08)
				(name "TUNE2")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 0)
				(length 5.08)
				(name "BAND")
				(number "5")
			)
			(pin no_connect line
				(at 0 -12.7 0)
				(length 5.08)
				(name "NC_1")
				(number "6")
			)
			(pin no_connect line
				(at 0 -15.24 0)
				(length 5.08)
				(name "NC_2")
				(number "7")
			)
			(pin passive line
				(at 0 -17.78 0)
				(length 5.08)
				(name "FMI")
				(number "8")
			)
			(pin power_in line
				(at 0 -20.32 0)
				(length 5.08)
				(name "RFGND")
				(number "9")
			)
			(pin power_in line
				(at 0 -22.86 0)
				(length 5.08)
				(name "GND_3")
				(number "10")
			)
			(pin power_in line
				(at 0 -25.4 0)
				(length 5.08)
				(name "GND_4")
				(number "11")
			)
			(pin passive line
				(at 0 -27.94 0)
				(length 5.08)
				(name "AMI")
				(number "12")
			)
			(pin output line
				(at 33.02 0 180)
				(length 5.08)
				(name "LOUT")
				(number "24")
			)
			(pin output line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "ROUT")
				(number "23")
			)
			(pin passive line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "DBYP")
				(number "22")
			)
			(pin power_in line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "VDD2")
				(number "21")
			)
			(pin power_in line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "VDD1")
				(number "20")
			)
			(pin passive line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "XTALI")
				(number "19")
			)
			(pin passive line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "XTALO")
				(number "18")
			)
			(pin input line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "SCLK")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "SDIO")
				(number "16")
			)
			(pin input line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "~{RST}")
				(number "15")
			)
			(pin power_in line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "GND_2")
				(number "14")
			)
			(pin power_in line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "GND_1")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SLW-1277545-2A-RA-S-D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 19.05 7.62 0)
		)
		(property "Value" "SLW-1277545-2A-RA-S-D"
			(at 19.05 5.08 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:SLW12775452ARASD"
			(at 19.05 -94.92 0)
		)
		(property "Datasheet" "https://www.sameskydevices.com/product/resource/supplyframepdf/slw-1277545-2a-ra-s-d.pdf"
			(at 19.05 -194.92 0)
		)
		(property "Description" "12.7 x 7.5 x 4.5 mm, 2 mm Raised Slide Actuator, Right Angle, Through Hole, Slide Switch"
			(at 0 0 0)
		)
		(property "Height" "5"
			(at 19.05 -394.92 0)
		)
		(property "Manufacturer" "Same Sky"
			(at 19.05 -694.92 0)
		)
		(property "Manufacturer PN" "SLW-1277545-2A-RA-S-D"
			(at 19.05 -794.92 0)
		)
		(symbol "SLW-1277545-2A-RA-S-D_0_1")
		(symbol "SLW-1277545-2A-RA-S-D_1_1"
			(pin passive line
				(at 0 -5.08 0)
				(length 5.08)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 0)
				(length 5.08)
				(name "CASE_GND")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 0)
				(length 5.08)
				(name "CASE_GND")
				(number "6")
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 22.86 -6.35 180)
				(length 5.08)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74AC595BQBR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 26.67 15.24 0)
		)
		(property "Value" "SN74AC595BQBR"
			(at 26.67 12.7 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:SN74AC595BQBR"
			(at 26.67 -87.3 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74ac595.pdf?ts=1722767931885&ref_url"
			(at 26.67 -187.3 0)
		)
		(property "Description" "Counter Shift Registers 1.5V to 6V, eight-bit shift registers with tri-state output registers"
			(at 15.24 17.78 0)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 26.67 -687.3 0)
		)
		(property "Manufacturer PN" "SN74AC595BQBR"
			(at 26.67 -787.3 0)
		)
		(symbol "SN74AC595BQBR_1_1"
			(pin input line
				(at 0 1.27 0)
				(length 5.08)
				(name "SRCLR")
				(number "10")
			)
			(pin input clock
				(at 0 -1.27 0)
				(length 5.08)
				(name "SRCLK")
				(number "11")
			)
			(pin input line
				(at 0 -3.81 0)
				(length 5.08)
				(name "RCLK")
				(number "12")
			)
			(pin input line
				(at 0 -6.35 0)
				(length 5.08)
				(name "OE")
				(number "13")
			)
			(pin input line
				(at 0 -8.89 0)
				(length 5.08)
				(name "SER")
				(number "14")
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin passive line
				(at 0 -16.51 0)
				(length 5.08)
				(name "EP")
				(number "17")
			)
			(pin power_in line
				(at 0 -19.05 0)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "QA")
				(number "15")
			)
			(pin output line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "QB")
				(number "1")
			)
			(pin output line
				(at 30.48 0 180)
				(length 5.08)
				(name "QC")
				(number "2")
			)
			(pin output line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "QD")
				(number "3")
			)
			(pin output line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "QE")
				(number "4")
			)
			(pin output line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "QF")
				(number "5")
			)
			(pin output line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "QG")
				(number "6")
			)
			(pin output line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "QH")
				(number "7")
			)
			(pin output line
				(at 30.48 -16.51 180)
				(length 5.08)
				(name "QH'")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74LV8T541PWR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.254 4.572 0)
		)
		(property "Value" "SN74LV8T541PWR"
			(at 7.874 1.524 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 13.97 -16.51 0)
		)
		(property "Datasheet" ""
			(at 13.97 -16.51 0)
		)
		(property "Description" "Level Shifter, Octal"
			(at 13.97 -13.97 0)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
		)
		(property "Manufacturer PN" "SN74LV8T541PWR"
			(at 0 0 0)
		)
		(symbol "SN74LV8T541PWR_0_0"
			(pin input line
				(at -2.54 -3.81 0)
				(length 2.54)
				(name "~{OE1}")
				(number "1")
			)
			(pin input line
				(at -2.54 -6.35 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -2.54 -8.89 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -2.54 -11.43 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin input line
				(at -2.54 -13.97 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin input line
				(at -2.54 -16.51 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin input line
				(at -2.54 -19.05 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin input line
				(at -2.54 -21.59 0)
				(length 2.54)
				(name "A7")
				(number "8")
			)
			(pin input line
				(at -2.54 -24.13 0)
				(length 2.54)
				(name "A8")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -26.67 0)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin input line
				(at 17.78 -3.81 180)
				(length 2.54)
				(name "~{OE2}")
				(number "19")
			)
			(pin output line
				(at 17.78 -6.35 180)
				(length 2.54)
				(name "Y1")
				(number "18")
			)
			(pin output line
				(at 17.78 -8.89 180)
				(length 2.54)
				(name "Y2")
				(number "17")
			)
			(pin output line
				(at 17.78 -11.43 180)
				(length 2.54)
				(name "Y3")
				(number "16")
			)
			(pin output line
				(at 17.78 -13.97 180)
				(length 2.54)
				(name "Y4")
				(number "15")
			)
			(pin output line
				(at 17.78 -16.51 180)
				(length 2.54)
				(name "Y5")
				(number "14")
			)
			(pin output line
				(at 17.78 -19.05 180)
				(length 2.54)
				(name "Y6")
				(number "13")
			)
			(pin output line
				(at 17.78 -21.59 180)
				(length 2.54)
				(name "Y7")
				(number "12")
			)
			(pin output line
				(at 17.78 -24.13 180)
				(length 2.54)
				(name "Y8")
				(number "11")
			)
			(pin power_in line
				(at 17.78 -26.67 180)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
		)
		(symbol "SN74LV8T541PWR_1_1")
		(embedded_fonts no)
	)
	(symbol "TPS2115ADRBR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "TPS2115ADRBR"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:TPS2115ADRBR"
			(at 26.67 -94.92 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tps2115a"
			(at 26.67 -194.92 0)
		)
		(property "Description" "Autoswitching Power Mux"
			(at 0 0 0)
		)
		(property "Height" "1"
			(at 26.67 -394.92 0)
		)
		(property "Mouser Part Number" "595-TPS2115ADRBR"
			(at 26.67 -494.92 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TPS2115ADRBR?qs=g%2FrhRe7LVpSXEuLZV5FMOQ%3D%3D"
			(at 26.67 -594.92 0)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 26.67 -694.92 0)
		)
		(property "Manufacturer PN" "TPS2115ADRBR"
			(at 26.67 -794.92 0)
		)
		(symbol "TPS2115ADRBR_1_1"
			(pin power_in line
				(at 0 0 0)
				(length 5.08)
				(name "IN2")
				(number "6")
			)
			(pin power_in line
				(at 0 -2.54 0)
				(length 5.08)
				(name "IN1")
				(number "8")
			)
			(pin passive line
				(at 0 -8.89 0)
				(length 5.08)
				(name "D0")
				(number "2")
			)
			(pin passive line
				(at 0 -11.43 0)
				(length 5.08)
				(name "D1")
				(number "3")
			)
			(pin open_collector line
				(at 0 -16.51 0)
				(length 5.08)
				(name "STAT")
				(number "1")
			)
			(pin power_out line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "OUT")
				(number "7")
			)
			(pin passive line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "ILIM")
				(number "4")
			)
			(pin power_in line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "GND_1")
				(number "5")
			)
			(pin power_in line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "GND_2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS63060DSCR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 22.86 0)
		)
		(property "Value" "TPS63060DSCR"
			(at 0 20.32 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:TPS63060DCSR"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "2.5V to 12V input voltage, 93% Efficient, 2.25A Switch Current Limit, Buck-Boost Converter"
			(at 0 0 0)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
		)
		(property "Package" "WSON-10 Texas Instruments"
			(at 0 0 0)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/TPS63060DSCR/Texas+Instruments/view-part/?ref=snap"
			(at 0 0 0)
		)
		(property "Manufacturer PN" "TPS63060DSCR"
			(at 0 0 0)
		)
		(symbol "TPS63060DSCR_0_0"
			(pin power_in line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "EN")
				(number "3")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "L1")
				(number "1")
			)
			(pin input line
				(at -17.78 0 0)
				(length 5.08)
				(name "PS/SYNC")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "VAUX")
				(number "6")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "PG")
				(number "5")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "VOUT")
				(number "9")
			)
			(pin power_in line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "GND")
				(number "7")
			)
		)
		(symbol "TPS63060DSCR_1_0"
			(pin passive line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "L2")
				(number "10")
			)
			(pin input line
				(at 17.78 -1.27 180)
				(length 5.08)
				(name "FB")
				(number "8")
			)
			(pin power_in line
				(at 17.78 -8.89 180)
				(length 5.08)
				(name "EP")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB4085-GF-A_REVB"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.588 20.828 0)
		)
		(property "Value" "USB4085-GF-A_REVB"
			(at -9.398 -41.148 0)
		)
		(property "Footprint" "FMRadioPartsFootprintLibrary:GCT_USB4085-GF-A_REVB"
			(at 2.54 24.13 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "USB Type C, THT"
			(at 0 0 0)
		)
		(property "PARTREV" "B"
			(at 0 0 0)
		)
		(property "SNAPEDA_PN" "USB4085-GF-A"
			(at 0 0 0)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.16mm"
			(at 0 0 0)
		)
		(property "Manufacturer" "Global Connector Technology"
			(at 2.54 24.13 0)
		)
		(property "Manufacturer PN" "USB4085-GF-A"
			(at 0 0 0)
		)
		(symbol "USB4085-GF-A_REVB_0_0"
			(pin power_out line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "VBUS")
				(number "A4")
			)
			(pin power_out line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "VBUS__2")
				(number "B4")
			)
			(pin power_out line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "VBUS__3")
				(number "B9")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "CC1")
				(number "A5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "CC2")
				(number "B5")
			)
			(pin bidirectional line
				(at -10.16 -3.81 0)
				(length 5.08)
				(name "D+1")
				(number "A6")
			)
			(pin bidirectional line
				(at -10.16 -6.35 0)
				(length 5.08)
				(name "D+2")
				(number "B6")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "D-1")
				(number "A7")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "D-2")
				(number "B7")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "SBU1")
				(number "A8")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "SBU2")
				(number "B8")
			)
			(pin power_in line
				(at -10.16 -24.13 0)
				(length 5.08)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -10.16 -26.67 0)
				(length 5.08)
				(name "GND__1")
				(number "A12")
			)
			(pin power_in line
				(at -10.16 -29.21 0)
				(length 5.08)
				(name "GND__2")
				(number "B1")
			)
			(pin power_in line
				(at -10.16 -31.75 0)
				(length 5.08)
				(name "GND__3")
				(number "B12")
			)
			(pin passive line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "SHELL")
				(number "S1")
			)
			(pin passive line
				(at -10.16 -35.56 0)
				(length 5.08)
				(hide yes)
				(name "SHELL__1")
				(number "S2")
			)
			(pin passive line
				(at -10.16 -35.56 0)
				(length 5.08)
				(hide yes)
				(name "SHELL__2")
				(number "S3")
			)
			(pin passive line
				(at -10.16 -35.56 0)
				(length 5.08)
				(hide yes)
				(name "SHELL__3")
				(number "S4")
			)
		)
		(symbol "USB4085-GF-A_REVB_1_0"
			(pin power_out line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "VBUS__1")
				(number "A9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "header_m_1x3_2.54mm"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.08 0)
		)
		(property "Value" "header_m_1x3_2.54mm"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
		)
		(property "Manufacturer PN" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "header_m_1x3_2.54mm_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
)
