(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "AD8592"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "AD8592"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_MO:MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-www.analog.com/media/en/technical-documentation/data-sheets/AD8591_8592_8594.pdf"
			(at 0 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*"
			(at 0 0 0)
		)
		(symbol "AD8592_0_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
		)
		(symbol "AD8592_1_1"
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~{SD}")
				(number "5")
			)
		)
		(symbol "AD8592_2_1"
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~{SD}")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
	)
)
